|  |
| --- |
| Declaration of Performance |
| DoP-Nr.: 1794 0000 |

|  |  |  |
| --- | --- | --- |
| 1. | Unique identification code of the product-type | BauderFLEX TA 600 |
| 2. | Intended use/es | Reinforced bitumen sheets for roof waterproofing |
| 3. | Manufacturer | Paul Bauder GmbH & Co. KG, Korntaler Landstrasse 63,  70499 Stuttgart, Germany |
| 4. | System/s of assessment and verification of constancy of performance of the construction product | System 2+ |
| 5. | Harmonised standard  Notified body | EN 13707: 2013  Gemeinschaft für Qualitätsüberwachung von Polymerbitumen- und Bitumenbahnen e.V.  Certification Body 1724 |

**6. Declared performance**

|  |  |  |  |
| --- | --- | --- | --- |
| **Essential characteristics** |  | **Performance** | **Harmonized technical**  **specification** |
| External fire performance a) |  | Broof(t1) | EN V 1187: 2012 |
| Reaction to fire |  | Class E | EN 13501-1: 2010 |
| Watertightness, Method B |  | passed |  |
| Tensile properties:  Max. Tensile force lenght  Max. Tensile force transverse  Elongation at max. tensile force lenght  Elongation at max. tensile force transverse | (N/50 mm) (N/50 mm) ( %)  ( %) | ≥ 550  ≥ 400  ≥ 20  ≥ 20 | EN 13707: 2013 |
| Flexibility at low temperature | (°C) | ≤ -20 |  |
| Hazardous Substances **b), c)** |  | Passed,  see 5.3 EN 13707 |  |

For all other characteristics according to EN 13707: NPD (no performance determined)

a) Determination of external fire performance is a system test. which can be influenced by system components, which are not produced or sold by Bauder GmbH, thus performance for each product can not be given.

b) Product does not contain asbestos or tar

c) Because there is no European test method for leaching of the products, no statement can be made

The performance of the product identified above is in conformity with the set of declared performance/s. This declaration of performance is issued, in accordance with Regulation (EU) No 305/211, under the sole responsibility of the manufacturer identified above.

Signed for and on behalf of the manufacturer by:



Andrew Mackenzie  
Managing Director

Ipswich, 06.01.2016