

‘13

|  |
| --- |
| DoP-Nr.: 2013-14963 |
| **Declaration of Performance**  According to annex lll of Regulation (EU) 305/2011 (construction products regulation)  date: 28-06-2013 |

Continuous rooflight, with/without upstand.

Intended use for daylighting for flat and/or inclined roofs.

Unique identification as per order number.

|  |  |  |  |
| --- | --- | --- | --- |
| **Essential characteristics** | **Performance** | **AVCP** | **hEN** |
| Resistance to upward load | NPD | System 3 | EN 14963 : 2006 |
| Resistance to downward load | NPD |
| Reaction to fire [1] | B-s1, d0 |
| Resistance to fire | NPD |
| External fire performance | NPD |
| Water tightness | NPD |
| Impact resistance | NPD |
| Thermal transmittance | NPD |
| Direct airborne sound insulation | NPD |
| Luminous transmittance | NPD |
| Air permeability | NPD |
| Durability | NPD |

[1] Notified body: 0833. Test report no. 329269 dated 08/06/2013 : NPD - no performance determined.

**The performance of the product identified with the above identification codes are in conformity with the relevant declared performances.**

**This declaration of performance is issued under the sole responsibility of the manufacturer Xtralite (Rooflights) ltd.**

Signed for and on behalf of the manufacturer by:

Paul Felgate, Research & Development Manager



01.07.13

.................. .....................................................................................................

(Date) (signature)